Sender : Philippe_J_Maier@phac-aspc.gc.ca
SpeedFan version : SpeedFan 4.27
Motherboard model : Shuttle SN26P w/ Asus EN7800GT SLI and NVRAID x3

*****************************

BIOS CopyRight : XPC    - 42302e31)Phoenix - Award WorkstationBIOS v6.00PGoC(Phoenix - Award WorkstationBIOS v6.00PG
BIOS Date : 09/07/05
BIOS Extended Info : 
BIOS Name : AT/AT COMPATIBLE

Windows NT Uniprocessor Free version 5.1.2600

1 processor(s)
Advanced Micro Devices AMD Athlon(tm) 64 Processor 3500+ family 15 model 17 stepping 0 brand 0 2210 MHz (128.0 Kb level 1 - 512.0 Kb level 2 - 0 bytes level 3)
Running at 2210 MHz
I Agree to receive beta versions : ON

*****************************

IT8712F on ISA at $290 Temp1 : 45.0   min=44.0   max=47.0   mean=45.0
IT8712F on ISA at $290 Temp2 : -55.0   min=-55.0   max=-50.0   mean=-54.6
IT8712F on ISA at $290 Temp3 : -55.0   min=-55.0   max=-55.0   mean=-55.0
IT8712F on ISA at $290 Fan1 : 3590   min=3516   max=3668   mean=3598
IT8712F on ISA at $290 Fan2 : 1520   min=1507   max=3516   mean=1526
IT8712F on ISA at $290 Fan3 : 0   min=0   max=0   mean=0
IT8712F on ISA at $290 Pwm1 : 100%   min=100%   max=100%   mean=100%
IT8712F on ISA at $290 Pwm2 : 100%   min=100%   max=100%   mean=100%
IT8712F on ISA at $290 Pwm3 : 10%   min=10%   max=100%   mean=10%
IT8712F on ISA at $290 Vcore1 : 1.38   min=1.38   max=1.39   mean=1.38
IT8712F on ISA at $290 Vcore2 : 1.50   min=1.50   max=1.52   mean=1.51
IT8712F on ISA at $290 +3.3V : 3.26   min=3.26   max=3.26   mean=3.26
IT8712F on ISA at $290 +5V : 5.11   min=5.11   max=5.13   mean=5.11
IT8712F on ISA at $290 +12V : 12.10   min=12.10   max=12.22   mean=12.13
IT8712F on ISA at $290 -12V : -11.79   min=-11.79   max=-11.79   mean=-11.79
IT8712F on ISA at $290 -5V : -0.48   min=-0.48   max=-0.43   mean=-0.48
IT8712F on ISA at $290 +5V : 5.13   min=5.13   max=5.13   mean=5.13
IT8712F on ISA at $290 Vbat : 3.01   min=3.01   max=3.01   mean=3.01
[$13]=$77  [$14]=$D0  [$15]=$7F  [$16]=$7F
[$17]=$0D  [$20]=$56  [$21]=$5E  [$22]=$CC
[$23]=$BE  [$24]=$BD  [$25]=$3F  [$26]=$A5
[$27]=$BF  [$28]=$BC
ADT7463 on nForce2 SMBus at $2E CPU : 49.8   min=45.3   max=54.5   mean=49.0
ADT7463 on nForce2 SMBus at $2E Local : 44.8   min=43.8   max=47.3   mean=44.7
ADT7463 on nForce2 SMBus at $2E Remote 2 : 41.5   min=37.8   max=52.8   mean=41.0
ADT7463 on nForce2 SMBus at $2E Fan1 : 1367   min=1297   max=3120   mean=1390
ADT7463 on nForce2 SMBus at $2E Fan2 : 0   min=0   max=0   mean=0
ADT7463 on nForce2 SMBus at $2E Fan3 : 736   min=728   max=2970   mean=736
ADT7463 on nForce2 SMBus at $2E Fan4 : 0   min=0   max=0   mean=0
ADT7463 on nForce2 SMBus at $2E Pwm1 : 10%   min=10%   max=70%   mean=20%
ADT7463 on nForce2 SMBus at $2E Pwm2 : 100%   min=100%   max=100%   mean=100%
ADT7463 on nForce2 SMBus at $2E Pwm3 : 10%   min=10%   max=70%   mean=20%
ADT7463 on nForce2 SMBus at $2E +2.5V : 0.00   min=0.00   max=0.00   mean=0.00
ADT7463 on nForce2 SMBus at $2E Vcore : 0.00   min=0.00   max=0.00   mean=0.00
ADT7463 on nForce2 SMBus at $2E +3.3V : 5.14   min=5.12   max=5.15   mean=5.14
ADT7463 on nForce2 SMBus at $2E +5V : 0.00   min=0.00   max=0.00   mean=0.00
ADT7463 on nForce2 SMBus at $2E +12V : 0.00   min=0.00   max=0.00   mean=0.00
LM75 on nForce2 SMBus at $4E Temp : 0.0   min=0.0   max=0.0   mean=0.0
ACPI on ISA at $0 Temp1 : 40.0   min=40.0   max=40.0   mean=40.0

*****************************

Temp1 --> active=OFF  chip=0  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=
Temp2 --> active=OFF  chip=0  index=2 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=
Temp3 --> active=OFF  chip=0  index=3 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=
System --> active=ON  chip=1  index=1 wanted=50  warning=60  offset=0  InTray=OFF Used pwms=
NBr --> active=ON  chip=1  index=2 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=1 
CPU --> active=ON  chip=1  index=3 wanted=50  warning=70  offset=0  InTray=ON Used pwms=4 6 
Temp --> active=OFF  chip=2  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=
Temp1 --> active=OFF  chip=3  index=1 wanted=40  warning=50  offset=0  InTray=OFF Used pwms=
NBr (3-w) --> active=ON  chip=0  index=1
Pwr Light --> active=ON  chip=0  index=2
HD Fan --> active=ON  chip=0  index=3
ICE Fan --> active=ON  chip=1  index=1
Fan2 --> active=OFF  chip=1  index=2
ICE Fan 2 --> active=ON  chip=1  index=3
Fan4 --> active=OFF  chip=1  index=4
NBr (3-w) --> active=ON  chip=0  index=1  min=10  max=100  variate=ON
Pwr Light --> active=ON  chip=0  index=2  min=10  max=100  variate=OFF
HD Fan --> active=ON  chip=0  index=3  min=10  max=100  variate=ON
ICE Fan --> active=ON  chip=1  index=1  min=10  max=100  variate=ON
Speed05 --> active=ON  chip=1  index=2  min=0  max=100  variate=OFF
ICE Fan 2 --> active=ON  chip=1  index=3  min=10  max=100  variate=ON
Vcore1 --> active=ON  chip=0  index=1
Vcore2 --> active=ON  chip=0  index=2
+3.3V --> active=ON  chip=0  index=3
+5V --> active=ON  chip=0  index=4
+12V --> active=ON  chip=0  index=5
-12V --> active=ON  chip=0  index=6
-5V --> active=ON  chip=0  index=7
+5V --> active=ON  chip=0  index=8
Vbat --> active=ON  chip=0  index=9
+2.5V --> active=OFF  chip=1  index=1
Vcore --> active=OFF  chip=1  index=2
+3.3V --> active=OFF  chip=1  index=3
+5V --> active=OFF  chip=1  index=4
+12V --> active=OFF  chip=1  index=5
Set Fans to 100% on exit : OFF
Debug Mode : ON
Use ISA : ON
Use SMB : ON
Scan PCI : ON
Scan SMB : ON
Slow SMB detection : ON
Detect SuperIO : ON
ASUS Card Detect : ON
DELL Support : OFF
Command line : "C:\Program Files\SpeedFan\speedfan.exe" /SLOWDETECT
Delta Fan Speed : 10

*****************************

Chipset : nVidia nForce4
SMBus Base Address : $1C40
SMBus Revision : A2
SMBus I/O Enabled : ON

*****************************

Bus : 00 Device: 00 Function : 00 --> 005E10DE Vendor : 10DE Device : 005E (rev A3) - <Unknown device>
00: 10DE 005E 0006 00B0 00A3 0580 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1297 5036 0000 0000 0044 0000 0000 0000 00FF 0000
40: 1297 5036 E008 01E0 0022 1111 00D0 0000 0623 807F 0003 0000 2000 0003 0000 0000
60: 0000 0000 0000 0000 0000 0000 3606 0000 4444 0000 09D0 0000 0000 0000 0088 0000
80: FF13 0088 00FA 0000 0003 0000 0061 0000 100E 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0101 0101 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0003 0000 8000 0000 0000 0000 0000 0000 0000 0000
E0: 0008 A801 0000 FEE0 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 01 Function : 00 --> 005010DE Vendor : 10DE Device : 0050 (rev A3) - <Unknown device>
00: 10DE 0050 000F 00A0 00A3 0601 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1297 5036 0000 0000 0000 0000 0000 0000 0000 0000
40: 1297 5036 F000 FEFF 3EFA 00FF 3EFA 00FF 3EFA 00FF 5A00 0262 0000 0100 0000 FFFF
60: 1001 0000 1401 0000 1801 0000 0000 FFF9 0010 FFFF 00C1 0000 0000 1904 D200 0180
80: 2009 1800 080D 0000 00C0 0100 0000 0000 0000 0000 0000 0000 6421 A987 BCDE 0000
A0: 0000 4110 0000 0000 0000 0000 0000 0000 0290 02EF 0000 0000 0000 0000 0000 0000
C0: 8235 0080 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 1414 0001 0000 00D0 3080 2000 4461 1144 FF5A BF5F 0000 C000 FF10 FFFF 0000 0730

Bus : 00 Device: 01 Function : 01 --> 005210DE Vendor : 10DE Device : 0052 (rev A2) - <Unknown device>
00: 10DE 0052 0001 00B0 00A2 0C05 0000 0080 DC01 0000 0000 0000 0000 0000 0000 0000
20: 1C01 0000 1C41 0000 0000 0000 1297 5036 0000 0000 0044 0000 0000 0000 0103 0103
40: 1297 5036 0001 C002 0000 0000 0000 0000 1C01 0000 1C41 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 02 Function : 00 --> 005A10DE Vendor : 10DE Device : 005A (rev A2) - <Unknown device>
00: 10DE 005A 0007 00B0 10A2 0C03 0000 0080 3000 D010 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1297 5036 0000 0000 0044 0000 0000 0000 0115 0103
40: 1297 5036 0001 FE02 0000 0000 0000 0000 0000 0000 471D 0040 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 FF00 FFFF 0B03 0730

Bus : 00 Device: 02 Function : 01 --> 005B10DE Vendor : 10DE Device : 005B (rev A3) - <Unknown device>
00: 10DE 005B 0006 00B0 20A3 0C03 0000 0080 0000 FEB0 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1297 5036 0000 0000 0044 0000 0000 0000 0216 0103
40: 1297 5036 800A 2098 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 2020 0001 6000 8518 3C03 013F 0000 0000 0000 0508 1000 8020 3D89 22B6 2577 0034
80: 0001 FE02 0000 0000 0000 0000 1615 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0001 0101 0000 E000 0000 0000 0000 0000 0033 2211 0044 0000 03FF 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 FF10 FFFF 0D05 0730

Bus : 00 Device: 06 Function : 00 --> 005310DE Vendor : 10DE Device : 0053 (rev F2) - <Unknown device>
00: 10DE 0053 0005 00B0 8AF2 0101 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
20: F001 0000 0000 0000 0000 0000 1297 5036 0000 0000 0044 0000 0000 0000 0000 0103
40: 1297 5036 0001 0002 0000 0000 0000 0000 F002 0001 0000 0000 A8A8 20A8 006A 2099
60: 0000 C000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 FF10 FFFF 0000 0730

Bus : 00 Device: 07 Function : 00 --> 005410DE Vendor : 10DE Device : 0054 (rev F3) - <Unknown device>
00: 10DE 0054 0007 00B0 85F3 0101 0000 0000 09F1 0000 0BF1 0000 0971 0000 0B71 0000
20: D801 0000 2000 D010 0000 0000 1297 5036 0000 0000 0044 0000 0000 0000 0117 0103
40: 1297 5036 0001 0002 0000 0000 0000 0000 5017 1503 0000 0000 0000 0000 0000 0000
60: 0000 0000 0C51 0000 0F08 4206 0000 0000 782C 40C4 1001 0000 1001 0000 0020 0020
80: 0000 C000 4000 08F6 0000 10A0 A000 08F2 0000 10A0 0000 0000 0006 1006 0000 0101
A0: 0150 7C00 0000 0000 0000 0000 BB33 02AA CC05 0084 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 000A 000A 0008 A802 000A 0402 0042 0000 0000 0000 000E 87B0
E0: 000A 0402 0042 0000 0000 0000 0B90 8110 0000 0000 0000 0000 FF00 FFFF 3B0C 0732

Bus : 00 Device: 08 Function : 00 --> 005510DE Vendor : 10DE Device : 0055 (rev F3) - <Unknown device>
00: 10DE 0055 0007 00B0 85F3 0101 0000 0000 09E1 0000 0BE1 0000 0961 0000 0B61 0000
20: C401 0000 1000 D010 0000 0000 1297 5036 0000 0000 0044 0000 0000 0000 0114 0103
40: 1297 5036 0001 0002 0000 0000 0000 0000 5017 1503 0000 0000 0000 0000 0000 0000
60: 0000 0000 0C51 0000 0F08 4206 0000 0000 782C 40C4 1001 0000 1001 0000 0020 0020
80: 0000 4000 6000 08F2 0000 1090 0000 0000 0000 0000 0000 0000 0006 1006 0000 0101
A0: 0150 7C00 0000 0000 0000 0000 BB33 02AA CC05 0084 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 000A 000A 0008 A802 000A 0402 0042 0000 0000 0000 000E 87A0
E0: 000A 0402 0042 0000 0000 0000 0000 0010 0000 0000 0000 0000 FF00 FFFF 3412 0732

Bus : 00 Device: 09 Function : 00 --> 005C10DE Vendor : 10DE Device : 005C (rev A2) - <Unknown device>
00: 10DE 005C 0107 00A0 01A2 0604 0000 0001 0000 0000 0000 0000 0500 2005 00F0 2280
20: FFF0 0000 FFF0 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0206
40: 0000 0007 0001 0002 0007 0000 0000 0144 0000 7FFE 0000 0000 1FFF 1FFF 0000 0000
60: 0000 0000 0003 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0600 0000 4700 FE00 0000 0000 0008 A800 0000 FEE0 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 10 Function : 00 --> 005710DE Vendor : 10DE Device : 0057 (rev A3) - <Unknown device>
00: 10DE 0057 0007 00B8 00A3 0680 0000 0000 0000 D010 B001 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1297 5036 0000 0000 0044 0000 0000 0000 0114 1401
40: 1297 5036 0001 FE02 0100 0000 000A 1000 6405 0084 0000 0000 0000 0000 0000 0000
60: 000F 0000 0008 A802 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0011 0000 FF40 FFFF 2304 0732

Bus : 00 Device: 11 Function : 00 --> 005D10DE Vendor : 10DE Device : 005D (rev A3) - <Unknown device>
00: 10DE 005D 0107 0010 00A3 0604 0008 0001 0000 0000 0000 0000 0400 0004 01F1 0000
20: FFF0 0000 FFF1 0001 0000 0000 0000 0000 0000 0000 0040 0000 0000 0000 0000 0006
40: 4801 F802 0000 0000 5805 0082 0000 0000 0000 0000 0000 0000 8008 A800 0000 FEE0
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0010 0141 04C0 0000 2810 0000 3421 0301 0000 1041 0C80 0040 01C0 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 24 Function : 00 --> 11001022 Vendor : 1022 Device : 1100 (rev 00) - Advanced Micro Devices Athlon 64 / Opteron HyperTransport Technology Configuration
00: 1022 1100 0000 0010 0000 0600 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0080 0000 0000 0000 0000 0000
40: 0101 0001 0101 0001 0101 0001 0101 0001 0101 0001 0101 0001 0101 0001 0101 0001
60: 0000 0000 00E4 0000 CC0F 0F00 000C 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0008 2101 0020 1111 0622 8075 0002 0000 0169 0161 0000 00FF 0007 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 24 Function : 01 --> 11011022 Vendor : 1022 Device : 1101 (rev 00) - Advanced Micro Devices Athlon 64 / Opteron Address Map
00: 1022 1101 0000 0000 0000 0600 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
40: 0003 0000 0000 007F 0000 0000 0001 0000 0000 0000 0002 0000 0000 0000 0003 0000
60: 0000 0000 0004 0000 0000 0000 0005 0000 0000 0000 0006 0000 0000 0000 0007 0000
80: 0003 00E0 FF80 00EF B003 00FE C080 00FE 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0A03 0000 0B00 0000 0003 0080 D300 00FE
C0: 0000 0000 0000 0000 1013 0000 F000 000F 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0003 FF00 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 24 Function : 02 --> 11021022 Vendor : 1022 Device : 1102 (rev 00) - Advanced Micro Devices Athlon 64 / Opteron DRAM Controller
00: 1022 1102 0000 0000 0000 0600 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
40: 0001 0000 2001 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: DE00 07E0 DE00 07E0 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0007 0000 0000 0000 4555 1482 0B31 0000 8E80 B805 0707 3E7B 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 9300 D0A7 00D7 0000 EFDF 0010 806F 01FB
C0: 8000 0000 0000 0000 0000 0000 0000 0000 0031 200E 2B72 1210 E2C0 A11A 0690 0080
E0: 0998 0130 6263 1858 C3A0 9002 0110 930A 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 00 Device: 24 Function : 03 --> 11031022 Vendor : 1022 Device : 1103 (rev 00) - Advanced Micro Devices Athlon 64 / Opteron Miscellaneous Control
00: 1022 1103 0000 0000 0000 0600 0000 0080 0000 0000 0000 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
40: 3BFF 0000 0040 0000 0000 0000 0000 0000 15F0 32B4 00A3 0000 0000 0000 BCC0 D3FD
60: 00FD 0000 0000 0000 00C0 0000 0000 0000 0111 5102 8011 5000 3800 0800 221B 0000
80: 0000 2307 2113 2113 0000 0000 0000 0000 0000 0000 0040 0000 5050 3A50 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 003F 2000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 A701 000D 0000 0000 0000 0000
E0: 0000 0000 0520 075F 0519 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 01 Device: 00 Function : 00 --> 009210DE Vendor : 10DE Device : 0092 (rev A1) - <Unknown device>
00: 10DE 0092 0007 0010 00A1 0300 0000 0000 0000 A000 000C 9000 0000 0000 0004 A100
20: 0000 0000 8001 0000 0000 0000 1043 81DB 0000 0000 0060 0000 0000 0000 0112 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 0001 0000 0001 0000 D6CE 0023 0000 0000
60: 6801 0002 0000 0000 7805 0080 0000 0000 0000 0000 0000 0000 0010 0001 04C0 0064
80: 2810 000A 4D01 0001 0008 1081 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 05 Device: 06 Function : 00 --> 17241412 Vendor : 1412 Device : 1724 (rev 01) - IC Ensemble, Inc. VT1720/24 Envy24PT/HT PCI Multi-Channel Audio Controller
00: 1412 1724 0005 0210 0001 0401 4000 0000 A001 0000 A401 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1297 5036 0000 0000 0080 0000 0000 0000 0112 0000
40: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0001 0401 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

Bus : 05 Device: 07 Function : 00 --> 30441106 Vendor : 1106 Device : 3044 (rev 80) - VIA Technologies Inc VT63061 VIA Fire II 1394a OHCI Link Layer Ctrlr1
00: 1106 3044 0007 0210 1080 0C00 2008 0000 0000 D000 A801 0000 0000 0000 0000 0000
20: 0000 0000 0000 0000 0000 0000 1106 3044 0000 0000 0050 0000 0000 0000 0113 2000
40: 0000 0000 0000 0000 0000 0000 0000 0000 0001 E402 0000 0000 0000 0000 0000 0000
60: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
80: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
A0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
C0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000
E0: 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000 0000

*****************************

ISA Dump from address $290 --> <IT8712F> (ISA at $0290) (No error)
00: 11 10 FF 00 00 00 00 00 00 00 20 5B 00 2F 6F FF   .......... [./o.
10: FF FF FF 77 D0 7F 7F 0D 00 00 FF FF FF FF FF FF   ...w............
20: 56 5E CC BE BD 3F A5 BF BC 2D C9 C9 9F 6F 6F 6F   V^...?...-...ooo
30: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
40: FF FF FF FF FF FF FF FF 2D FF FF FF FF FF FF FF   ........-.......
50: FF 38 7F 7F 7F FF 5D 75 90 5D FA 12 80 00 00 00   .8....]u.]......
60: 7F 7F 7F 00 00 FF FF FF 7F 7F 7F 00 00 FF FF FF   ................
70: 7F 7F 7F 00 00 FF FF FF FF FF FF FF FF FF FF FF   ................
80: 11 10 00 00 00 00 00 00 00 00 20 5B 00 2F 6F FF   .......... [./o.
90: FF FF FF 77 D0 7F 7F 0D 00 00 FF FF FF FF FF FF   ...w............
A0: 56 5E CC BE BD 3F A5 BF BC 2D C9 C9 9F 6F 6F 6F   V^...?...-...ooo
B0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
C0: FF FF FF FF FF FF FF FF 2D FF FF FF FF FF FF FF   ........-.......
D0: FF 38 7F 7F 7F FF 5D 75 90 5D FA 12 80 00 00 00   .8....]u.]......
E0: 7F 7F 7F 00 00 FF FF FF 7F 7F 7F 00 00 FF FF FF   ................
F0: 7F 7F 7F 00 00 FF FF FF FF FF FF FF FF FF FF FF   ................

*****************************

SMB Dump from address $50 --> <RAM> (SMBus at $1C00) (No error)
00: 80 08 07 0D 0B 02 40 00 04 50 70 00 82 08 00 01   ......@..Pp.....
10: 0E 04 08 01 02 20 C0 60 70 00 00 48 28 48 28 80   ..... .`p..H(H(.
20: 60 60 40 40 00 00 00 00 00 3C 46 28 28 32 00 00   ``@@.....<F((2..
30: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01 AA   ................
40: 7F 7F 7F 7F B0 00 00 00 00 4F 43 5A 34 30 30 31   .........OCZ4001
50: 30 32 34 56 33 20 20 20 20 20 20 00 00 00 00 00   024V3      .....
60: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
80: 05 0B 16 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
90: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
A0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
B0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
C0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
D0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
E0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
F0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
SMB Dump from address $51 --> <RAM> (SMBus at $1C00) (No error)
00: 80 08 07 0D 0B 02 40 00 04 50 70 00 82 08 00 01   ......@..Pp.....
10: 0E 04 08 01 02 20 C0 60 70 00 00 48 28 48 28 80   ..... .`p..H(H(.
20: 60 60 40 40 00 00 00 00 00 3C 46 28 28 32 00 00   ``@@.....<F((2..
30: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 01 AA   ................
40: 7F 7F 7F 7F B0 00 00 00 00 4F 43 5A 34 30 30 31   .........OCZ4001
50: 30 32 34 56 33 20 20 20 20 20 20 00 00 00 00 00   024V3      .....
60: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
80: 05 0B 16 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
90: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
A0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
B0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
C0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
D0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
E0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
F0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
SMB Dump from address $53 --> <RAM> (SMBus at $1C00) (No error)
00: 00 30 1B BA AE D2 FF FF FF FF FF FF FF FF FF FF   .0..............
10: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
20: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
30: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
40: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
50: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
60: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
70: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
80: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
90: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
A0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
B0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
C0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
D0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
E0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
F0: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF   ................
SMB Dump from address $2E --> <ADT7463> (SMBus at $1C40) (No error)
00: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
10: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
20: 00 00 C5 00 00 32 2C 2D 2D 0F FF FF AF 1C 00 00   .....2,--.......
30: 1A FF 1A 64 64 64 00 00 00 00 00 00 00 27 41 6A   ...ddd.......'Aj
40: 85 00 00 1F 00 FF 00 FF 00 FF 00 FF 00 FF 81 7F   ................
50: 81 7F 81 3F FF FF FF FF FF FF FF FF E2 E2 E2 C4   ...?............
60: C4 EC 2E 0E 80 80 80 5A 5A 20 64 64 3F 44 40 00   .......ZZ dd?D@.
70: 00 00 B4 00 00 00 20 68 47 FF 00 55 00 01 00 00   ...... hG..U....
80: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
90: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
A0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
B0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
C0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
D0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
E0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
F0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
SMB Dump from address $4E --> <LM75> (SMBus at $1C40) (No error)
00: 00 00 00 06 06 00 00 00 00 00 00 00 00 00 00 00   ................
10: 00 00 FF 0F 00 00 00 00 00 00 00 00 00 00 00 00   ................
20: 00 00 00 00 00 00 00 00 83 12 12 28 00 00 00 00   ...........(....
30: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
40: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
50: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
60: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
70: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
80: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
90: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
A0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
B0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
C0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
D0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
E0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................
F0: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00   ................

*****************************

Retry attempts info for SMBus at $1C00
  [ -1]=482
  [  0]=234
  [  1]=248
Retry attempts info for SMBus at $1C40
  [ -1]=484
  [  0]=240
  [  1]=244

*****************************

Scanning SMBus at $1C00...
Decoding DIMM #0
 Memory type is DDR
 Module Rows : 2
 Levels : 2.5V
 Parity : NO PARITY
 Refresh Rate : 7.8us
 Total Size : 1024MB
Decoding DIMM #1
 Memory type is DDR
 Module Rows : 2
 Levels : 2.5V
 Parity : NO PARITY
 Refresh Rate : 7.8us
 Total Size : 1024MB
Scanning SMBus at $1C40...

*****************************

Scanning SMBus at $1C00...
 - device found at $08
 - device found at $50
 - device found at $51
 - device found at $53
Scanning SMBus at $1C40...
 - device found at $08
 - device found at $2E
 - device found at $4E

*****************************

Can change fan speeds : YES
Can smoothly change fan speeds : YES
Can stop fans : NO

*****************************

WMI interface is registered : ON
MB manufacturer: Shuttle Inc
MB model: FN26V10
MB version:  
ACPI temp: 40.0
ACPI active trip point: 0.0
ACPI passive trip point: 73.0
ACPI critical trip point: 75.0
WMI quick analysis results -->
EXPLORING : root\CIMV2\Win32_BaseBoard
  -> Object Start
  Caption = Base Board
  CreationClassName = Win32_BaseBoard
  Description = Base Board
  HostingBoard = True
  Manufacturer = Shuttle Inc
  Name = Base Board
  PoweredOn = True
  Product = FN26V10
  SerialNumber =  
  Tag = Base Board
  Version =  
  Method -> IsCompatible(ElementToCheck)
EXPLORING : root\WMI\msacpi_thermalzonetemperature
  -> Object Start
  Active = True
  ActiveTripPoint =  0 0 0 0 0 0 0 0 0 (0.0C)
  ActiveTripPointCount = 1
  CriticalTripPoint = 3482 (75.0C)
  CurrentTemperature = 3132 (40.0C)
  InstanceName = ACPI\ThermalZone\THRM_0
  PassiveTripPoint = 3462 (73.0C)
  Reserved = 1
  SamplingPeriod = 60
  ThermalConstant1 = 4
  ThermalConstant2 = 3
  ThermalStamp = 6
EXPLORING : root\CIMV2\CIM_AssociatedSensor
EXPLORING : root\CIMV2\CIM_CoolingDevice
EXPLORING : root\CIMV2\CIM_Fan
EXPLORING : root\CIMV2\CIM_HeatPipe
EXPLORING : root\CIMV2\CIM_ManagementController
EXPLORING : root\CIMV2\CIM_NumericSensor
EXPLORING : root\CIMV2\CIM_PackageAlarm
EXPLORING : root\CIMV2\CIM_PackageCooling
EXPLORING : root\CIMV2\CIM_Refrigeration
EXPLORING : root\CIMV2\CIM_Sensor
EXPLORING : root\CIMV2\CIM_Tachometer
EXPLORING : root\CIMV2\CIM_TemperatureSensor
EXPLORING : root\CIMV2\CIM_VoltageSensor
EXPLORING : root\CIMV2\Win32_CurrentProbe
EXPLORING : root\CIMV2\Win32_Fan
EXPLORING : root\CIMV2\Win32_HeatPipe
EXPLORING : root\CIMV2\Win32_Refrigeration
EXPLORING : root\CIMV2\Win32_TemperatureProbe
EXPLORING : root\CIMV2\Win32_VoltageProbe
EXPLORING : SMBIOS
  -> Object Start
<-- End of WMI quick analysis results

*****************************

DMI structures from SMBIOS ver. 2.2
MBManufacturer : Shuttle Inc
MBModel : FN26V10
MBVersion : 
BIOSVendor : Phoenix Technologies, LTD
BIOSVersion : 6.00 PG
Structure   0 - 0000 - fixed len is 15 bytes -> BIOS information
  -> 01 02 00 E0 03 07 90 9E CB 7F 00 00 00 00 33
  -> 'Phoenix Technologies, LTD'
  -> '6.00 PG'
  -> '09/07/2005'
Structure   1 - 0001 - fixed len is 21 bytes -> System information
  -> 01 02 03 04 12 97 F5 25 FF FF FF FF FF FF FF FF FF FF FF FF 06
  -> 'Shuttle Inc'
  -> 'SN26V10'
  -> ' '
  -> ' '
Structure   2 - 0002 - fixed len is 4 bytes -> Base board (or module) information
  -> 01 02 03 04
  -> 'Shuttle Inc'
  -> 'FN26V10'
  -> ' '
  -> ' '
Structure   3 - 0003 - fixed len is 9 bytes -> System enclosure or chassis
  -> 01 03 02 03 04 02 02 02 02
  -> ' '
  -> ' '
  -> ' '
  -> ' '

*****************************

0 events defined

*****************************

Tray icon size : 16x16
UPTIME : 0 days 17:23:13

*****************************

Win9x:NO  64Bit:NO  GiveIO:YES  SpeedFan:YES
I/O properly initialized
Linked ISA BUS at $0290
Linked nVidia nForce4 SMBUS at $1C00
Linked nVidia nForce4 SMBUS at $1C40
Scanning ISA BUS at $0290...
IT8712F/IT8705F found on ISA at $290
SuperIO Chip=IT8712F
Scanning nForce2 SMBus at $1C00...
Address $14 appears to be WRITE ONLY...
Address $15 appears to be WRITE ONLY...
Address $16 appears to be WRITE ONLY...
Address $17 appears to be WRITE ONLY...
Address $18 appears to be WRITE ONLY...
Address $19 appears to be WRITE ONLY...
Address $1A appears to be WRITE ONLY...
Address $1B appears to be WRITE ONLY...
Address $1C appears to be WRITE ONLY...
Address $1D appears to be WRITE ONLY...
Address $1E appears to be WRITE ONLY...
Address $1F appears to be WRITE ONLY...
Address $20 appears to be WRITE ONLY...
Address $21 appears to be WRITE ONLY...
Address $22 appears to be WRITE ONLY...
Address $23 appears to be WRITE ONLY...
Address $24 appears to be WRITE ONLY...
Address $25 appears to be WRITE ONLY...
Address $26 appears to be WRITE ONLY...
Address $27 appears to be WRITE ONLY...
Address $28 appears to be WRITE ONLY...
Address $29 appears to be WRITE ONLY...
Address $2A appears to be WRITE ONLY...
Address $2B appears to be WRITE ONLY...
Address $2C appears to be WRITE ONLY...
Address $2D appears to be WRITE ONLY...
Address $2E appears to be WRITE ONLY...
Address $2F appears to be WRITE ONLY...
Address $30 appears to be WRITE ONLY...
Address $31 appears to be WRITE ONLY...
Address $32 appears to be WRITE ONLY...
Address $33 appears to be WRITE ONLY...
Address $34 appears to be WRITE ONLY...
Address $35 appears to be WRITE ONLY...
Address $36 appears to be WRITE ONLY...
Address $37 appears to be WRITE ONLY...
Address $38 appears to be WRITE ONLY...
Address $39 appears to be WRITE ONLY...
Address $3A appears to be WRITE ONLY...
Address $3B appears to be WRITE ONLY...
Address $3C appears to be WRITE ONLY...
Address $3D appears to be WRITE ONLY...
Address $3E appears to be WRITE ONLY...
Address $3F appears to be WRITE ONLY...
Address $40 appears to be WRITE ONLY...
Address $41 appears to be WRITE ONLY...
Address $42 appears to be WRITE ONLY...
Address $43 appears to be WRITE ONLY...
Address $44 appears to be WRITE ONLY...
Address $45 appears to be WRITE ONLY...
Address $46 appears to be WRITE ONLY...
Address $47 appears to be WRITE ONLY...
Address $48 appears to be WRITE ONLY...
Address $49 appears to be WRITE ONLY...
Address $4A appears to be WRITE ONLY...
Address $4B appears to be WRITE ONLY...
Address $4C appears to be WRITE ONLY...
Address $4D appears to be WRITE ONLY...
Address $4E appears to be WRITE ONLY...
Address $4F appears to be WRITE ONLY...
Address $73 appears to be WRITE ONLY...
Address $77 appears to be WRITE ONLY...
Scanning nForce2 SMBus at $1C40...
Address $14 appears to be WRITE ONLY...
Address $15 appears to be WRITE ONLY...
Address $16 appears to be WRITE ONLY...
Address $17 appears to be WRITE ONLY...
Address $18 appears to be WRITE ONLY...
Address $19 appears to be WRITE ONLY...
Address $1A appears to be WRITE ONLY...
Address $1B appears to be WRITE ONLY...
Address $1C appears to be WRITE ONLY...
Address $1D appears to be WRITE ONLY...
Address $1E appears to be WRITE ONLY...
Address $1F appears to be WRITE ONLY...
Address $20 appears to be WRITE ONLY...
Address $21 appears to be WRITE ONLY...
Address $22 appears to be WRITE ONLY...
Address $23 appears to be WRITE ONLY...
Address $24 appears to be WRITE ONLY...
Address $25 appears to be WRITE ONLY...
Address $26 appears to be WRITE ONLY...
Address $27 appears to be WRITE ONLY...
Address $28 appears to be WRITE ONLY...
Address $29 appears to be WRITE ONLY...
Address $2A appears to be WRITE ONLY...
Address $2B appears to be WRITE ONLY...
Address $2C appears to be WRITE ONLY...
Address $2D appears to be WRITE ONLY...
ADT7463 (ID=$27) found on SMBus at $2E
Address $2F appears to be WRITE ONLY...
Address $30 appears to be WRITE ONLY...
Address $31 appears to be WRITE ONLY...
Address $32 appears to be WRITE ONLY...
Address $33 appears to be WRITE ONLY...
Address $34 appears to be WRITE ONLY...
Address $35 appears to be WRITE ONLY...
Address $36 appears to be WRITE ONLY...
Address $37 appears to be WRITE ONLY...
Address $38 appears to be WRITE ONLY...
Address $39 appears to be WRITE ONLY...
Address $3A appears to be WRITE ONLY...
Address $3B appears to be WRITE ONLY...
Address $3C appears to be WRITE ONLY...
Address $3D appears to be WRITE ONLY...
Address $3E appears to be WRITE ONLY...
Address $3F appears to be WRITE ONLY...
Address $40 appears to be WRITE ONLY...
Address $41 appears to be WRITE ONLY...
Address $42 appears to be WRITE ONLY...
Address $43 appears to be WRITE ONLY...
Address $44 appears to be WRITE ONLY...
Address $45 appears to be WRITE ONLY...
Address $46 appears to be WRITE ONLY...
Address $47 appears to be WRITE ONLY...
Address $48 appears to be WRITE ONLY...
Address $49 appears to be WRITE ONLY...
Address $4A appears to be WRITE ONLY...
Address $4B appears to be WRITE ONLY...
Address $4C appears to be WRITE ONLY...
Address $4D appears to be WRITE ONLY...
LM75 found on SMBus at $4E
Address $4F appears to be WRITE ONLY...
Address $50 appears to be WRITE ONLY...
Address $73 appears to be WRITE ONLY...
Address $77 appears to be WRITE ONLY...
Found ACPI temperature (40.0C)
End of detection
Error loading event -->
  CfgVersion=01.0001
  EventsVersion=01.0001
Loaded 0 events

*****************************

Win9x:NO  64Bit:NO  GiveIO:YES  SpeedFan:YES
SpeedFan.sys ver. 1.001
I/O properly initialized
Linked ISA BUS at $0290
Linked PCI
Starting PCI scan...
Linked nVidia nForce4 SMBUS at $1C00
nForce2 SMBus at $1C00 returned <No error>
Linked nVidia nForce4 SMBUS at $1C40
SMBus at $1C40 WRITEQ failed ($0A)
nForce2 SMBus at $1C40 returned <no ack>
PCI scan done!
Scanning ISA BUS at $0290...
About to check DELL support
PCI scanning is enabled
End of DELL support check
IT8712F/IT8705F found on ISA at $290
  --> [$13]=$77
  --> [$14]=$D0
  --> [$15]=$7F
  --> [$16]=$7F
  --> [$17]=$0D
  --> FAN_CTL1 is set to PWM=$7F
  --> FAN_CTL2 is set to PWM=$7F
  --> FAN_CTL3 is set to PWM=$0D
 -> Temperature sensor diode 1 : Thermistor
 -> Temperature sensor diode 2 : Thermistor
 -> Temperature sensor diode 3 : Thermistor
 -> FAN1 divisor : 8
 -> FAN2 divisor : 8
 -> FAN3 divisor : 8
 -> PWM 1 mode : Software controlled
 -> PWM 2 mode : Software controlled
 -> PWM 3 mode : Software controlled
 -> PWMOUT clock : 3M
 -> Temperature 1 offset : 0
 -> Temperature 2 offset : 0
 -> Temperature 3 offset : 0
 -> FAN1 mult : 1
 -> FAN1 div : 1
 -> FAN2 mult : 1
 -> FAN2 div : 1
 -> FAN3 mult : 1
 -> FAN3 div : 1
 -> Reverse PWM01 logic : OFF
 -> Reverse PWM02 logic : OFF
 -> Reverse PWM03 logic : OFF
Second pass...
ITE r[$20]=$87 r[$21]=$12 r[$22]=$06 r[$07]=$01 
NEW --> SuperIO chip=ITE IT8712F ($002E)
Checking $0370 for SMSC (2)...
Checking $0370 for SMSC (1)...
Checking $03F0 for SMSC (2)...
Checking $03F0 for SMSC (1)...
Checking $002E for SMSC (1)...
Registers [$002E] : $87 $12 $00 $00
Checking $004E for SMSC (1)...
Checking $002E for WINBOND...
$002E --> Device ID=$87 Revision=$12
Checking $004E for WINBOND...
Checking $0250 for WINBOND...
Checking $0370 for WINBOND...
Checking $03F0 for WINBOND...
Checking $002E for NS...
Checking $004E for NS...
Checking $002E for ITE (1)...
Registers [$002E] : $87 $12 $06
SuperIO Chip=IT8712F
 --> [$25]=$00
 --> [$26]=$00
 --> [$27]=$00
 --> [$28]=$00
 --> [$29]=$00
 --> [$2A]=$01
 --> LDN0 [$60]=$03F0 [$62]=$0000 [$64]=$0000 (enabled)
 --> LDN1 [$60]=$03F8 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN2 [$60]=$0000 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN3 [$60]=$0378 [$62]=$0000 [$64]=$0080 (enabled)
 --> LDN4 [$60]=$0290 [$62]=$0000 [$64]=$0000 (enabled)
 --> LDN5 [$60]=$0060 [$62]=$0064 [$64]=$0000 (enabled)
 --> LDN6 [$60]=$0000 [$62]=$0000 [$64]=$0000 (enabled)
 --> LDN7 [$60]=$0000 [$62]=$0800 [$64]=$0000 (disabled)
 --> LDN8 [$60]=$0300 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDN9 [$60]=$0201 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDNA [$60]=$0310 [$62]=$0000 [$64]=$0000 (disabled)
 --> LDNB [$60]=$0000 [$62]=$0000 [$64]=$0000 (disabled)
Scanning nForce2 SMBus at $1C00...
Address $14 appears to be WRITE ONLY...
Address $15 appears to be WRITE ONLY...
Address $16 appears to be WRITE ONLY...
Address $17 appears to be WRITE ONLY...
Address $18 appears to be WRITE ONLY...
Address $19 appears to be WRITE ONLY...
Address $1A appears to be WRITE ONLY...
Address $1B appears to be WRITE ONLY...
Address $1C appears to be WRITE ONLY...
Address $1D appears to be WRITE ONLY...
Address $1E appears to be WRITE ONLY...
Address $1F appears to be WRITE ONLY...
Address $20 appears to be WRITE ONLY...
Address $21 appears to be WRITE ONLY...
Address $22 appears to be WRITE ONLY...
Address $23 appears to be WRITE ONLY...
Address $24 appears to be WRITE ONLY...
Address $25 appears to be WRITE ONLY...
Address $26 appears to be WRITE ONLY...
Address $27 appears to be WRITE ONLY...
Address $28 appears to be WRITE ONLY...
Address $29 appears to be WRITE ONLY...
Address $2A appears to be WRITE ONLY...
Address $2B appears to be WRITE ONLY...
Address $2C appears to be WRITE ONLY...
Address $2D appears to be WRITE ONLY...
Address $2E appears to be WRITE ONLY...
Address $2F appears to be WRITE ONLY...
Address $30 appears to be WRITE ONLY...
Address $31 appears to be WRITE ONLY...
Address $32 appears to be WRITE ONLY...
Address $33 appears to be WRITE ONLY...
Address $34 appears to be WRITE ONLY...
Address $35 appears to be WRITE ONLY...
Address $36 appears to be WRITE ONLY...
Address $37 appears to be WRITE ONLY...
Address $38 appears to be WRITE ONLY...
Address $39 appears to be WRITE ONLY...
Address $3A appears to be WRITE ONLY...
Address $3B appears to be WRITE ONLY...
Address $3C appears to be WRITE ONLY...
Address $3D appears to be WRITE ONLY...
Address $3E appears to be WRITE ONLY...
Address $3F appears to be WRITE ONLY...
Address $40 appears to be WRITE ONLY...
Address $41 appears to be WRITE ONLY...
Address $42 appears to be WRITE ONLY...
Address $43 appears to be WRITE ONLY...
Address $44 appears to be WRITE ONLY...
Address $45 appears to be WRITE ONLY...
Address $46 appears to be WRITE ONLY...
Address $47 appears to be WRITE ONLY...
Address $48 appears to be WRITE ONLY...
Address $49 appears to be WRITE ONLY...
Address $4A appears to be WRITE ONLY...
Address $4B appears to be WRITE ONLY...
Address $4C appears to be WRITE ONLY...
Address $4D appears to be WRITE ONLY...
Address $4E appears to be WRITE ONLY...
Address $4F appears to be WRITE ONLY...
Address $73 appears to be WRITE ONLY...
Address $77 appears to be WRITE ONLY...
Scanning nForce2 SMBus at $1C40...
Address $14 appears to be WRITE ONLY...
Address $15 appears to be WRITE ONLY...
Address $16 appears to be WRITE ONLY...
Address $17 appears to be WRITE ONLY...
Address $18 appears to be WRITE ONLY...
Address $19 appears to be WRITE ONLY...
Address $1A appears to be WRITE ONLY...
Address $1B appears to be WRITE ONLY...
Address $1C appears to be WRITE ONLY...
Address $1D appears to be WRITE ONLY...
Address $1E appears to be WRITE ONLY...
Address $1F appears to be WRITE ONLY...
Address $20 appears to be WRITE ONLY...
Address $21 appears to be WRITE ONLY...
Address $22 appears to be WRITE ONLY...
Address $23 appears to be WRITE ONLY...
Address $24 appears to be WRITE ONLY...
Address $25 appears to be WRITE ONLY...
Address $26 appears to be WRITE ONLY...
Address $27 appears to be WRITE ONLY...
Address $28 appears to be WRITE ONLY...
Address $29 appears to be WRITE ONLY...
Address $2A appears to be WRITE ONLY...
Address $2B appears to be WRITE ONLY...
Address $2C appears to be WRITE ONLY...
Address $2D appears to be WRITE ONLY...
ADT7463 (ID=$27) found on SMBus at $2E
 -> PWM 1 mode : Manually controlled
 -> PWM 2 mode : Manually controlled
 -> PWM 3 mode : Manually controlled
 -> PWMOUT1 clock : 35.3Hz
 -> PWMOUT2 clock : 35.3Hz
 -> PWMOUT3 clock : 35.3Hz
 -> Temperature 1 offset : 0
 -> Temperature 2 offset : 0
 -> Temperature 3 offset : 0
 -> FAN1 mult : 1
 -> FAN1 div : 1
 -> FAN2 mult : 1
 -> FAN2 div : 1
 -> FAN3 mult : 1
 -> FAN3 div : 1
 -> FAN4 mult : 1
 -> FAN4 div : 1
 -> Reverse PWM01 logic : OFF
 -> Reverse PWM02 logic : OFF
 -> Reverse PWM03 logic : OFF
Address $2F appears to be WRITE ONLY...
Address $30 appears to be WRITE ONLY...
Address $31 appears to be WRITE ONLY...
Address $32 appears to be WRITE ONLY...
Address $33 appears to be WRITE ONLY...
Address $34 appears to be WRITE ONLY...
Address $35 appears to be WRITE ONLY...
Address $36 appears to be WRITE ONLY...
Address $37 appears to be WRITE ONLY...
Address $38 appears to be WRITE ONLY...
Address $39 appears to be WRITE ONLY...
Address $3A appears to be WRITE ONLY...
Address $3B appears to be WRITE ONLY...
Address $3C appears to be WRITE ONLY...
Address $3D appears to be WRITE ONLY...
Address $3E appears to be WRITE ONLY...
Address $3F appears to be WRITE ONLY...
Address $40 appears to be WRITE ONLY...
Address $41 appears to be WRITE ONLY...
Address $42 appears to be WRITE ONLY...
Address $43 appears to be WRITE ONLY...
Address $44 appears to be WRITE ONLY...
Address $45 appears to be WRITE ONLY...
Address $46 appears to be WRITE ONLY...
Address $47 appears to be WRITE ONLY...
Address $48 appears to be WRITE ONLY...
Address $49 appears to be WRITE ONLY...
Address $4A appears to be WRITE ONLY...
Address $4B appears to be WRITE ONLY...
Address $4C appears to be WRITE ONLY...
Address $4D appears to be WRITE ONLY...
LM84 configuration register=$06 ($4E)
MAX1617 configuration byte=$06 ($4E)
Probing MAX6657 at $4E
LM75 found on SMBus at $4E
 -> Temperature 1 offset : 0
Address $4F appears to be WRITE ONLY...
Address $50 appears to be WRITE ONLY...
Address $73 appears to be WRITE ONLY...
Address $77 appears to be WRITE ONLY...
About to probe TOSHIBA SUPPORT...
End of TOSHIBA SUPPORT probing
About to probe SCSI...
End of SCSI probing
About to probe UGURU support...
Motherboard is Shuttle Inc FN26V10
End of UGURU support probing
About to probe ACPI temperatures...
Found ACPI temperature (40.0C)
 -> Temperature 1 offset : 0
End of ACPI temperatures probing
End of detection
Reading Cfg Version 2.01
Old sensor properly detected -->
  IT8712F on ISA @ $290
PROP PWM 2 mode (14) = Software controlled
PROP PWM 3 mode (19) = Software controlled
PROP PWM 1 mode (13) = Software controlled
Old sensor properly detected -->
  ADT7463 on nForce2 SMBus @ $2E
PROP PWM 1 mode (13) = Manually controlled
PROP PWM 3 mode (19) = Manually controlled
PROP PWM 2 mode (14) = Manually controlled
Old sensor properly detected -->
  LM75 on nForce2 SMBus @ $4E
Old sensor properly detected -->
  ACPI on ISA @ $0
PWM from IT8712F@$290(onISA@$290) -->
  NBr (3-w) 10 100
  properly added
PWM from IT8712F@$290(onISA@$290) -->
  Pwr Light 10 100
  properly added
PWM from IT8712F@$290(onISA@$290) -->
  HD Fan 10 100
  properly added
PWM from ADT7463@$2E(onSMBusnForce2@$1C40) -->
  ICE Fan 10 100
  properly added
PWM from ADT7463@$2E(onSMBusnForce2@$1C40) -->
  Speed05 0 100
  properly added
PWM from ADT7463@$2E(onSMBusnForce2@$1C40) -->
  ICE Fan 2 10 100
  properly added
Temperature from IT8712F@$290(onISA@$290) -->
  Temp1 40 50 0
  properly added
Temperature from IT8712F@$290(onISA@$290) -->
  Temp2 40 50 0
  properly added
Temperature from IT8712F@$290(onISA@$290) -->
  Temp3 40 50 0
  properly added
Temperature from ADT7463@$2E(onSMBusnForce2@$1C40) -->
  System 50 60 0
  properly added
Temperature from ADT7463@$2E(onSMBusnForce2@$1C40) -->
  NBr 40 50 0
  PWM 1 from 0
  properly added
Temperature from ADT7463@$2E(onSMBusnForce2@$1C40) -->
  CPU 50 70 0
  PWM 1 from 1
  PWM 3 from 1
  properly added
Temperature from LM75@$4E(onSMBusnForce2@$1C40) -->
  Temp 40 50 0
  properly added
Temperature from ACPI -->
  Temp1 40 50 0
  properly added
Fan from IT8712F@$290(onISA@$290) -->
  NBr (3-w)
  properly added
Fan from IT8712F@$290(onISA@$290) -->
  Pwr Light
  properly added
Fan from IT8712F@$290(onISA@$290) -->
  HD Fan
  properly added
Fan from ADT7463@$2E(onSMBusnForce2@$1C40) -->
  ICE Fan
  properly added
Fan from ADT7463@$2E(onSMBusnForce2@$1C40) -->
  Fan2
  properly added
Fan from ADT7463@$2E(onSMBusnForce2@$1C40) -->
  ICE Fan 2
  properly added
Fan from ADT7463@$2E(onSMBusnForce2@$1C40) -->
  Fan4
  properly added
Volt from IT8712F@$290(onISA@$290) -->
  Vcore1
  properly added
Volt from IT8712F@$290(onISA@$290) -->
  Vcore2
  properly added
Volt from IT8712F@$290(onISA@$290) -->
  +3.3V
  properly added
Volt from IT8712F@$290(onISA@$290) -->
  +5V
  properly added
Volt from IT8712F@$290(onISA@$290) -->
  +12V
  properly added
Volt from IT8712F@$290(onISA@$290) -->
  -12V
  properly added
Volt from IT8712F@$290(onISA@$290) -->
  -5V
  properly added
Volt from IT8712F@$290(onISA@$290) -->
  +5V
  properly added
Volt from IT8712F@$290(onISA@$290) -->
  Vbat
  properly added
Volt from ADT7463@$2E(onSMBusnForce2@$1C40) -->
  +2.5V
  properly added
Volt from ADT7463@$2E(onSMBusnForce2@$1C40) -->
  Vcore
  properly added
Volt from ADT7463@$2E(onSMBusnForce2@$1C40) -->
  +3.3V
  properly added
Volt from ADT7463@$2E(onSMBusnForce2@$1C40) -->
  +5V
  properly added
Volt from ADT7463@$2E(onSMBusnForce2@$1C40) -->
  +12V
  properly added
Error loading event -->
  CfgVersion=01.0001
  EventsVersion=01.0001
Loaded 0 events
Preparing report...